**Battery Acid Spill Protocol**

1. Inform your safety captain of the spill immediately.
2. Isolate and evacuate the area surrounding the spill.
3. Wear all protective gear, including goggles and gloves. Secure all free-hanging materials.
4. Remove baking soda from the chemical spill kit. Sprinkle small amount of baking soda onto the spill to neutralize the battery acid.
5. Keep adding baking soda until the spill stops bubbling.
6. Seal the battery in a plastic bag, making sure it is secure for disposal.
7. Clean area of the spill, wiping away any excess baking soda. Ensure that the area is completely free of any residual battery acid or baking soda.
8. Follow safe disposal procedures for battery disposal. Refer to team safety manual for detailed instructions if necessary.